Embraer 170 PROCEDURES

For detailed instructions on how to fly this aircraft, see the Aircraft Handbook. For suggested speeds, see the Reference tab.


____________________________________
BEFORE START

[ ] Parking Brake -- SET
     (press CTRL+PERIOD key)

____________________________________
ENGINE START

Press CTRL+E to initiate engine autostart sequence.

____________________________________
AFTER START

[ ] Engine Start Switches -- CHECK GEN
[ ] Pitot Heat -- ON
[ ] De-ice -- AS REQUIRED
[ ] Engine Start Levers -- CHECK IDLE
[ ] Lights -- AS REQUIRED
[ ] Autopilot -- SET and OFF
[ ] Instruments -- CHECKED
[ ] Autobrake Switch -- RTO (Rejected Takeoff)
[ ] Avionics Switch -- ON
[ ] Avionics -- SET
     (press SHIFT+2 to display radio stack)

____________________________________
DURING TAXI/BEFORE TAKEOFF

[ ] Brakes -- RELEASE
     (press PERIOD key)
[ ] Thrust Levers-- INCREASE SLIGHTLY TO ROLL
    (press F3 or F2 as necessary)
[ ] Thrust Levers -- IDLE FOR TAXI
    (press F2 or F3 as necessary)
[ ] Flight Controls -- CHECK
[ ] Flaps -- SET FOR TAKEOFF (5)
     (press F7 as necessary)
[ ] Brakes -- SET
     (press PERIOD key)

____________________________________
CLEARED FOR TAKEOFF

[ ] Engine Start Switches -- GEN
[ ] Flight Director -- ON
[ ] Autothrottle -- ARM
     (if using TO/GA mode for takeoff)
[ ] Transponder -- ON
     (press SHIFT+2 to display radio stack)
[ ] Lights -- AS REQUIRED

____________________________________
TAKEOFF

[ ] Brakes -- RELEASE
     (press PERIOD key)
[ ] Thrust Levers -- ADVANCE SMOOTHLY TO 40% N1
     (wait for engine stabilization)
     (press F2 or F3 as necessary)
[ ] Thrust Levers -- ADVANCE SMOOTHLY TO 100% N1
     (press F2 or F3 as necessary)
     --or--
     TO/GA Mode -- Engage
          (press CTRL+SHIFT+R)
[ ] Engine Instruments -- MONITOR
[ ] Airspeed 80 KIAS -- CALLOUT "80 KNOTS"
                                    -- VERIFY PROPER THRUST SET
[ ] Airspeed V1 -- CALLOUT "V1"
[ ] Airspeed VR -- CALLOUT "ROTATE"
                           -- ROTATE TO APPROX. 10 DEGREES PITCH UP
[ ] Airspeed V2 -- CALLOUT "V2"
[ ] Landing Gear -- UP (WHEN POSITIVE CLIMB ESTABLISHED)
     (press G)
[ ] Airspeed --MAINTAIN V2+20 KIAS
[ ] Autopilot -- ENGAGE AT 1,000' AGL
[ ] Flaps-- RETRACT TO 1 AT 1,000' AGL
    (press F6 until 1)
[ ] Flaps-- UP AT 210 KIAS
    (press F6 until Up)
[ ] Autothrottle -- OFF
[ ] Thrust Levers-- 90% N1
    (press F2 or F3 as necessary)
[ ] Airspeed -- 250 KIAS AT 3,000' AGL
[ ] Landing Gear Lever -- Verify OFF

____________________________________
CLIMB

[ ] Airspeed -- MAINTAIN 250 KIAS
[ ] Landing Lights -- OFF ABOVE 10,000' MSL
[ ] Airspeed -- 280 KIAS ABOVE 10,000' MSL
[ ] Altimeter -- SET TO 29.92 CROSSING 18,000' MSL

____________________________________
CRUISE

[ ] Thrust Levers-- AS DESIRED
    (press F2 or F3 as necessary)
[ ] Trim -- AS NECESSARY
     (press Num Pad 1 or Num Pad 7 as necessary)

____________________________________
DESCENT

[ ] Autobrake Switch -- AS DESIRED
[ ] Airspeeds (VREF, VAPP) -- COMPUTED and SET
     (see the Reference tab of the Kneeboard)
[ ] De-ice -- AS REQUIRED
[ ] Autopilot -- AS DESIRED
[ ] Thrust Levers -- AS DESIRED
    (press F2 or F3 as necessary)
[ ] Altimeter -- SET TO LOCAL SETTING CROSSING 18,000' MSL
[ ] Avionics -- SET
     (press SHIFT+2 to display radio stack)
[ ] Airspeed -- <250 KIAS BELOW 10,000' MSL
[ ] Landing Lights -- ON BELOW 10,000' MSL
[ ] Approach Procedure -- REVIEW

____________________________________
APPROACH

[ ] Airspeed -- AS DESIRED
[ ] Thrust Levers -- AS DESIRED
    (press F2 or F3 as necessary)
[ ] Flaps -- AS DESIRED
     (press F7 as necessary)
[ ] Autopilot -- AS DESIRED
[ ] Autothrottle -- ARM
     (if using TO/GA mode for go-around)

____________________________________
LANDING

[ ] Airspeed -- AS DESIRED
[ ] Thrust Levers -- AS DESIRED
    (press F2 or F3 as necessary)
[ ] Speedbrake -- ARMED
     (press SHIFT + / [FORWARD SLASH key])
[ ] Landing Gear -- DOWN AND CONFIRMED
     (press G)
[ ] Flaps -- AS DESIRED
     (press F7 as necessary)
[ ] Start Switches -- GEN
[ ] Autopilot -- AS DESIRED

____________________________________
LANDING ROLL

[ ] Thrust Levers -- IDLE
    (press F2 or F3 as necessary)
[ ] Autopilot -- CHECK DISENGAGED
[ ] Autothrottle -- CHECK OFF
[ ] Speedbrake Lever -- CHECK FULL UP
     (press SHIFT+/ [FORWARD SLASH key] if necessary)
[ ] Brake -- AS NECESSARY
     (press PERIOD key)
[ ] Thrust Levers-- REVERSE
     (press F2 until Reverse)
[ ] Thrust Levers -- IDLE AT 60 KIAS
     (press F3 until Idle)

____________________________________
TAXI-IN

[ ] Speedbrake Lever -- DN
     (press / [FORWARD SLASH key])
[ ] Flap Lever -- UP
     (press F6 until Up)
[ ] Pitot Heat -- OFF
[ ] Engine Start Switches -- OFF
[ ] Landing Lights -- AS DESIRED
[ ] Flight Director -- OFF
[ ] Transponder -- AS REQUIRED

____________________________________
PARKING

[ ] Parking Brake -- SET
     (press CTRL+PERIOD)
[ ] Start Levers -- CUTOFF
     (press CTRL+SHIFT+F1)
[ ] De-ice -- OFF
[ ] Lights -- AS REQUIRED
[ ] Speedbrake Lever -- DOWN
     (press / [FORWARD SLASH key] if necessary)
[ ] Transponder -- AS REQUIRED

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator 2002. To learn about using, printing, and customizing checklists, see Help.