Embraer 170 REFERENCE INFORMATION

For detailed instructions on how to fly this aircraft, see the Aircraft Handbook. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel
           135,844 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel.

VMO - Maximum Operating Speed (airspeed)
           340 KIAS

MMO - Maximum Operating Speed (Mach)
           .82 Mach

Turbulent Air Penetration Speed
           280 KIAS/.73 Mach

VLO - Maximum Gear Operating Speed
           235 KIAS

VLE - Maximum Landing Gear Extension Speed
           270 KIAS/.82 Mach

Maximum Flap (Placard) Speeds
             Flaps      KIAS
              1	230
	2	230
	5	225
	10	210
	15	195
	25	190
	30	185
	40	158

V1 - Takeoff Decision Speed (dry runway; flaps 5)
       Standard temperature, sea level pressure altitude
             150 KIAS (143,000 lbs)
             143 KIAS (132,000 lbs)
       Standard temperature, 5,000' pressure altitude
             152 KIAS (143,000 lbs)
             145 KIAS (132,000 lbs)

VR - Rotation Speed (dry runway, flaps 5)
       Standard temperature, sea level pressure altitude
             154 KIAS (143,000 lbs)
             147 KIAS (132,000 lbs)
       Standard temperature, 5,000' pressure altitude
             157 KIAS (143,000 lbs)
             149 KIAS (132,000 lbs)

V2 - Takeoff Safety Speed (dry runway, flaps 5)
       Standard temperature, sea level pressure altitude
             162 KIAS (143,000 lbs)
             155 KIAS (132,000 lbs)
       Standard temperature, 5,000' pressure altitude
             161 KIAS (143,000 lbs)
             155 KIAS (132,000 lbs)

VREF - Landing Approach Speed (flaps 30, gear down)
             147 KIAS (136,400 lbs)
             144 KIAS (132,000 lbs)


NOTE:  For explanations of speeds used on this tab, see "V-speeds" in the Glossary section of Help.