McDonnell Douglas F/A-18A Hornet

Wingspan: 40 feet 5 inches
Length: 56 feet 
Height: 15 feet 4 inches

AN/APG-73 Programable Radar

Propulsion: F404-GE-400 
Thrust: 16,000 lbs
Airflow: 146 lb/sec
Weight: 2,282 lb 
Length: 154 in  
Inlet Diameter: 31 in    
Maximum Diameter: 35 in
Pressure Ratio: 26 to 1

Weights: 
BOW               23,832 lbs. 
Max Payload       13,700 lbs.
Default Payload   13,284 lbs see (aircraft.cfg)
Max ZFW           38,410 lbs.
Internal Fuel     10,860 lbs.(1644 gal)
External Fuel      6,730 lbs.(1019 gal)   
Max Fuel          17,590 lbs.(2663 gal)
Default MGTOW     55,584 lbs. 
Max MGTOW         56,000 lbs.

Speeds:
Max speed, Mil power Mach 1.0 
Econ: 36,089 ft. Mach 1.7 
Max Speed: Mach 1.8+
Landing speed 134 knots

Combat radius, interdiction, hi-lo-lo-hi 290 nm 
Combat endurance, CAP 150 nm from aircraft carrier 1 h 45 min 
Ferry range, unrefueled More than 1,800 nm 
Cieling: 50,000 ft.

Minimum wind over deck: 
Launching 35 knots 
Recovery 19 knots 

Landing gear:

Dowty retractable tricycle type, with twin-wheel nose and single-wheel
350 lb/sq in for carrier operations, 
200 lb/sq in for land operations.

Armament: 9 load stations

Internal:  

M61A1 Vulcan 20 mm Gatling Gun
Feed System: 270 lbs 
Gun: 252 lbs  
Ammunition: 319 lbs 
Total: 841 lbs  

Air-to-air missiles:

AIM-7 Sparrow 
Primary Function: Air-to-air guided missile
Contractor: Raytheon Co.
Power Plant: Hercules MK-58 solid-propellant rocket motor
Thrust: Classified
Speed: Classified
Range: Classified
Length: 12 ft 
Diameter: 8 inches 
Wingspan: 3 ft, 4 inches
Warhead: Annular blast fragmentation warhead
Launch Weight: 500 lbs
Guidance System: Raytheon semiactive on either continuous wave or pulsed Doppler radar energy
Date Deployed: AIM-7F, 1976; AIM-7M, 1982
Unit Cost: Approximately $125,000
Inventory: Classified

AIM-9 Sidewinders
Primary Function: Air-to-air missile
Contractor: Raytheon Co.; Ford Aerospace and Communications Corp.; Loral
Power Plant: Thiokol Hercules and Bermite MK 36 Mod 11; single-stage, solid-propellant rocket motor
Length: 9 ft 6 inches
Diameter: 5 inches
Fin Span: 2 ft 1 inch
Speed: Supersonic
Warhead: Blast fragmentation (conventional) weighing 20.8 pounds (9.36 kg)
Launch Weight: 190 
Range: 8.7 nm
Guidance System: Solid-state infrared homing system
Unit Cost: $41,300
Date Deployed: 1956

6 AIM- 20 AMRAM
Primary Function: Medium-range, air-to-air tactical missile
Contractor: Hughes/Raytheon
Power Plant: High performance, directed rocket motor
Length: 12 feet 
Launch Weight: 335 lbs 
Diameter: Seven inches 
Wing Span: 21 inches 
Speed: Supersonic
Warhead: Blast Fragmentation; high explosive
Unit Cost: $386,000
Date Deployed: September 1991

Air-to-ground weapons:

AGM-65E Maverick
Seeker: TV with
magnification
Speed: Mach 0.65
Length: 8 ft 2 in
Weight: 464 lbs
Warhead: 125 lbs
shaped charge
Range: 0.6 to 14 nm
Diameter:
Drag factor: 46

AGM-84D Harpoon
Primary Function: Anti-ship cruise missile.
Contractor: The Boeing Company
Power Plant: Teledyne Turbojet 
Thrust: 660 lbs 
Length: 12 ft, 7 inches 
Weight: 1,145 lbs
Diameter: 13.5 inches 
Wing Span: 3 ft
Range: Over-the-horizon, in excess of 60 nautical miles.
Speed: High Subsonic
Guidance: Sea-skimming cruise monitored by radar altimeter, active radar terminal homing.
Warhead: Penetration high-explosive blast at 488 lbs
Unit Cost: $720,000
Date Deployed: 1985


HGM-88 HARM
Primary Function: Air-to-surface anti-radiation missile.
Contractor: Raytheon
Power Plant: Thiokol dual-thrust, solid propellent, rocket motor
Length: 13 ft, 8 inches
Launch Weight: 800 lbs 
Diameter: 10 inches 
Wing Span: 3 ft, 8 inches 
Range: 57+ nm
Speed: 1,216 kmph
Guidance: radar homing
Warhead: Blast fragmentation; warhead weight 150 lbs
Unit Cost: $284,000
Date Deployed: 1985

Mk82
Type: 500 lb class general-purpose iron bomb
Length: 7 ft 2 in
Weight: 531 lbs
Warhead: 275 lbs H-6 high-explosive
Drag factor: 40

Mk82HD Snakeye
Type: 500 lb class high-drag iron bomb 
Length: 7 ft 6 in
Weight: 570 lbs
Warhead: 275 lbs H-6 high-explosive
Drag factor: 40

Mk83
Type: 1,000 lb class general-purpose iron bomb
Length: 9 ft 11 in
Weight: 985 lbs
Warhead: 416 lbs H-6 high-explosive
Drag factor: 50

Mk84
Type: 2,000 lb class general-purpose iron bomb
Length: 12 ft 9 in
Weight: 1,972 lbs
Warhead: 945 lbs H-6 high-explosive
Drag factor: 60

GBU-15 Guided Bomb Unit
Type: TV guided bomb
Length: 12 ft 10 in
Weight: 2,510 lbs
Warhead: 945 lbs H-6 high-explosive
Range: 5 miles
Drag factor: 46                 

CBU-84 Cluster Bomb Unit
Type: Sub-munitions dispenser
Length: 7 ft 8 in
Weight: 960 lbs
Warhead: 202 combined-effect bomblets
Drag factor: 50

BLU-107/B Durandal
Type: Anti-runway cratering bomb
Length: 8 ft 2 in
Weight: 450 lbs
Warhead: 330 lbs high-explosive
Drag factor: 40