Handley Page HP137 PROCEDURES

For suggested speeds, see the Reference tab.

____________________________________
BEFORE STARTING ENGINE

[ ] Battery (ON)
[ ] Nav Lights (ON)
[ ] Endtry Door (CLOSED)
[ ] No Smoking Sign (ON)
[ ] Seat Belt Sign (ON)
[ ] Avionics Master Switch (OFF)
[ ] Fuel Quantity (Checked)
[ ] Fuel Crossfeed Valve (CLOSED)
[ ] Parking Brake (SET)

____________________________________
ENGINE START

Press CTRL+E to initiate engine autostart sequence, or:

[ ] Power Levers (IDLE)
[ ] Propellor Levers (FULL FORWARD)
[ ] Condition Levers (HIGH IDLE)
[ ] Beacons (ON)
[ ] Right Ignition and Engine Start Switch (ON)
	(click and hold until engine starts)
[ ] Right Condition Lever (LOW IDLE)
	(after the N1 Turbine RPM has stabilized, 30% minimum)
[ ] Left Ignition and Engine Start Switch (ON)
	(click and hold until engine starts)
[ ] Left Condition Lever (LOW IDLE)
	(after the N1 Turbine RPM has stabilized, 30% minimum)
[ ] Generators (ON)
[ ] Avionic Master Switch (ON)

____________________________________
BEFORE TAXI

[ ] ATC Clearance (OBTAIN)
[ ] Altimeters (SET)
[ ] Right Ignition and Engine Start Switch (CHECK OFF)
[ ] Left Ignition and Engine Start Switch (CHECK OFF)

____________________________________
TAXI

[ ] Trim (SET)
[ ] Flaps (10°)
[ ] Anti-Ice (AS REQUIRED)
[ ] Pitot Heat (AS REQUIRED)

____________________________________
BEFORE TAKEOFF

[ ] Flight Controls (CHECKED)
[ ] Transponder (ALTITUDE)
[ ] Propellor Levers (FULL FORWARD)
[ ] Condition Levers (HIGH IDLE)
[ ] Taxi Lights (OFF)
[ ] Landing Lights (ON)
[ ] Strobe Lights (ON)

____________________________________
AFTER TAKEOFF

[ ] Gear (UP)
[ ] Flaps (0°)
[ ] Propeller Synchrophaser (OFF)
[ ] Landing Lights (OFF)

____________________________________
CRUISE

[ ] Power Levers (AS REQUIRED)
[ ] Propellor Levers (AS REQUIRED)
[ ] Condition Levers (AS REQUIRED)
[ ] Fuel Crossfeed Valve (CLOSED)
[ ] Anti-Ice (AS REQUIRED)
[ ] Pitot Heat (AS REQUIRED)

____________________________________
DESCENT

[ ] Power Levers (AS REQUIRED)
[ ] Propellor Levers (AS REQUIRED)
[ ] Condition Levers (AS REQUIRED)
[ ] Anti-Ice (AS REQUIRED)
[ ] Pitot Heat (AS REQUIRED)
[ ] Altimeter (SET)
[ ] Landing Lights (ON)

____________________________________
BEFORE LANDING

[ ] Landing Gear (3 GREEN)
[ ] Flaps (AS REQUIRED)
[ ] Propellor Levers (FULL FORWARD)
[ ] Condition Levers (HIGH IDLE)
[ ] Fuel Crossfeed Valve (CLOSED)
[ ] Propeller Synchrophaser (OFF)

____________________________________
AFTER LANDING

[ ] Anti-Ice (AS REQUIRED)
[ ] Pitot Heat (AS REQUIRED)
[ ] Transponder (STANDYBY)
[ ] Strobe Lights (OFF)
[ ] Landing Lights (OFF)
[ ] Taxi Lights (ON)

____________________________________
SECURING AIRPLANE

[ ] Parking Brake (SET)
[ ] Taxi Lights (OFF)
[ ] Beacons (OFF)
[ ] Avionics Master Switch (OFF)
[ ] Propellor Levers (AS REQUIRED)
[ ] Left Generator (OFF)
[ ] Left Condition Lever (FUEL CUTOFF)
[ ] Right Generator (OFF)
[ ] Right Condition Lever (FUEL CUTOFF)
[ ] Nav Lights (OFF)
[ ] Master Switch (OFF)