LONG BEACH AIRPORT (DAUGHERTY FIELD)
California, USA
ICAO IDENTIFIER:  KLGB
Terminal Information

Elevation:	57' 
Mag Var: 13.8E
ATIS:	126.00
LGB Tower:	120.50  (Rwy 12)  119.40 (Rwy 30)
LGB Ground:	133.00
LGB Clearance Del:	118.15

NAVAIDS:

NDB:	LG 233.00 BECCA LOM Rwy 30


RUNWAY INFORMATION

		Length		Width		OBS Hdg		Navaid		Approach
								 Freq		Lighting
								 	
Rwy 12/30		10,000'		 200'	12	    121		VASI 4 bars 3degs	None
					30	    301		110.30	I-LGB	MALSR
					HIRL - No runway centerline lighting
					Runway surface: Concrete
					
Runway 30 ILS: descend to 1600ft by MIDDS (IAF) and depart heading 255 degs intercept the localiser and descend via the ILS to landing (g/s active at Outer Marker BECCA at 1600ft (I-LGB 4.1NM) Middle Marker - (I-LGB 0.5NM))


Rwy 7R/25L	 5,420'		 150'	7R	     76		None		None
					25L	    256		VASI 4 bars 4degs	None
					MIRL No runway centerline lighting
					Runway surface: Asphalt
					
Rwy 7L/25R	 6,192'		 150'	7L	     76		None		None
					25R	    256		VASI 4 bars 4degs	None
					MIRL - No runway centerline lighting
					Runway surface: Asphalt
					
Rwy 16R/34L	 4,470'		  75'	16R	    166		VASI 4 bars 4degs	Strobes
					34L	    346				None
					MIRL - No runway centerline lighting
					Runway surface: Asphalt

Rwy 16L/34R	 4,267'		  75'	16L	    166		None		None
					34R	    346		None		Strobes
					MIRL - No runway centerline lighting
					Runway surface: Asphalt
					
Runway 16R/34L and 16L/34R certified for light aircraft traffic only - Visual approaches in use.



Enjoy!

Shehryar Ansari
shez@attglobal.net