SANTA ANA JOHN WAYNE ORANGE COUNTY AIRPORT
California, USA
ICAO IDENTIFIER:  KSNA
Terminal Information

Elevation:	54' 
Mag Var: 13.7E
ATIS:	126.00
SNA Tower:	126.80  379.90
SNA Ground:	120.80
SNA Clearance Del:	118.00  121.85

NAVAIDS:

NDB:	NA 337.00 MAAGG 19R


RUNWAY INFORMATION

		Length		Width		OBS Hdg		Navaid		Lighting
								 Freq
								 	
Rwy 1L/19R	 5700'		150'	1L	    014		VASI		None
					19R	    194		111.75	I-SNA	MALSR
					19R LDA	    181		108.30	I-OJW	MALSR
					19R			VASI
					HIRL - No runway centerline lighting
					Runway surface: Asphalt
					
Runway 19R ILS:		descend to 3500ft and depart POM vor (IAF) radial 144 intercept the localiser at SAGER intersection descend to 3300ft then 			descend via the ILS to landing (Outer Marker - LEMON (I-SNA 7.6), Middle Marker - MAAGG (I-SNA 0.5))

Runway 19R LDA Approach:	intercept the LDA on heading 136 at EFFIE fix at 3000ft descend with the LDA until visual with runway, join final approach 			course hdg 194 to landing.

Runway 1L Localiser 
Back Course Approach:	descend to 2000ft intercept the localiser on a heading 050 at NEWPO (IAF), descend visually via VASI to landing.

				

Rwy 1R/19L	 2887'		 75'	1R	    014		None		None
					19L	    194		VASI		None
					MIRL - No runway centerline lighting
					Runway surface: Asphalt
					
Runway 1R/19L certified for light aircraft traffic only - Visual approaches in use.



Enjoy!

Shehryar Ansari
shez@attglobal.net