BOEING 777-300 REFERENCE INFORMATION

For detailed instructions on how to fly this aircraft, see the Aircraft Handbook. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel
           580,069 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel.

VMO - Maximum Operating Speed (airspeed)
           330 KIAS

MMO - Maximum Operating Speed (Mach)
            .84 Mach

Turbulent Air Penetration Speed
           280 KIAS/.84 Mach

VLO - Maximum Gear Operating Speed
           270 KIAS/.82 Mach

VLE - Maximum Landing Gear Extension Speed
           270 KIAS/.82 Mach

Maximum Flap (Placard) Speeds
              Flaps      KIAS
              1	255
	5	235
	15	215
	20	200
	25	190
	30	180

V1 - Takeoff Decision Speed
        Standard temperature, sea-level pressure altitude
              153 KIAS (580,000 lbs)
        Standard temperature, 3,000' pressure altitude
              154 KIAS (580,000 lbs)

VR - Rotation Speed (dry runway; flaps 5)
        Standard temperature, sea level pressure altitude
              156 KIAS (580,000 lbs)
        Standard temperature, 3,000' pressure altitude
              157 KIAS (580,000 lbs)

V2 - Takeoff Safety Speed (dry runway; flaps 5)
        Standard temperature, sea level pressure altitude
              162 KIAS (580,000 lbs)
        Standard temperature, 3,000' pressure altitude
              162 KIAS (580,000 lbs)

VREF - Landing Approach Speed (flaps 30; gear down)
             157 KIAS (580,000 lbs)


NOTE:  For explanations of speeds used on this tab, see "V-speeds" in the Glossary section of Help.