Pilot Series Checklist Boeing 777-200 Full Version for FS2000 
Component of The Pilot Series Checklist Part IV
Made by Chris van Bijlert
http://fly.to/pilotserieschecklist

____________________________________
      COCKPIT PREPARATION
____________________________________
Initial Cockpit Preparation

- Airplane Power Source: CHECK
- Battery Switch: ON
- Hydraulic Panel: SET
- Landing Gear Lever: DOWN
- Alternate Flaps Arm Switch: OFF
- Alternate Flaps Selector: OFF
- Bus Tie Switches: AUTO
- Electrical Power: ESTABLISHED
- Cockpit Lighting: AS REQUIRED
- Pack Switches: AUTO
- Airplane Number: VERIFY
- Overhead Maintenance Panel: CHECK
- Cargo Temperature Selectors: AS REQUIRED
- Circuit Breakers: CHECK
- Spare Bulbs: CHECK
- Emergency Equipment: CHECK
- ADIRU: VERIFY ON
- Exterior Lights: SET
- Service Items: CHECK
- Electronic Checklist: CHECK

- Initial Cockpit Preparation: COMPLETED

____________________________________
Company COMM and FMC Initialization - CAPTAIN

- MFD, CO COMM Reset: ACCOMPLISHED
- MFD, CO COMM (ACARS): Select, Initialize
- CDU, IDENT Page: VERIFY DATA
- CDU, POS INIT 1/3: SELECT
- CDU, ADIRS Present Position: ENTER
- CDU, FMC Route: ENTER
- CDU, RTE and LEGS Page: VERIFY

- Company COMM and FMC Initialization - CAPTAIN: COMPLETED

____________________________________
Cockpit Preparation - CAPTAIN

- Left Wiper Selector: OFF
- Electrical Panel: CHECK
- Drive Disc Switches: CHECK
- Backup GEN Switch: ON
- Generator Control Switches: ON
- Bus Tie Switches: AUTO
- Battery Switch: CHECK ON
- Thrust Asym Comp: AUTO
- Primary Flight Computers: AUTO
- ADIRU: VERIFY

- Emergency Exit Light Switch: ARMED
- Service Interphone Switch: OFF
- Passenger Oxygen Switch: OFF
- Window Heat: ON
- Ram Air Turbine Switch: OFF
- C1, C2 Electrical Primary Hydraulic Pump Switches: OFF
- Engine Primary Hydraulic Pump Switch: ON
- C1, C2 Air, Left Electrical Hydraulic Demands Pumps: OFF

- No Smoking Selector: ON
- Seat Belts Selector: OFF
- OVHD/CB Light Control: AS DESIRED
- Dome Light Control: AS DESIRED
- Storm Light Control: AS DESIRED
- Master Brightness Knob: AS DESIRED
- Glareshield Panel Knob: AS DESIRED

- Landing Light Switches: OFF
- Runway Turnoff, Taxi, Strobe Light Switches: OFF
- Beacon Light Switch: OFF
- NAV Light Switch: ON
- Logo, Wing Light Switches: AS REQUIRED
- Indicator Light Switches: TEST, AS DESIRED

- Engine Anti-Ice Selectors: AUTO
- Wing Anti-Ice Selectors: AUTO
- Fuel Pump Switches: OFF
- Crossfeed Switches, FWD, AFT: OPEN, THEN CLOSE
- Fuel Jettison: OFF
- Fuel To Remain Knob: IN
- Fuel Jettison Arm Switch: OFF
- Auto Start Switch: ON
- Start/Ignition Selectors: NORMAL
- EEC Mode Switches: NORMAL

- APU Fire Handle: IN
- APU BTL Disch. Light: VERIFY OFF
- Fire/OVHT Test Switch: TEST
- Cargo Fire Disch. Light: VERIFY OFF
- Cargo Fire Arm Switches: OFF

- Equipment Cooling Switch: AUTO
- Gasper Switch: ON
- Recirc. Fan Switches: ON
- FLT Deck Temp Control: AUTO RANGE
- Cabin Temp Control: Mid Position

- Pack Switches: AUTO
- Trim Air Switches: ON
- Bleed Air ISLN Switches: AUTO
- Left, Right ENG Bleed Switch: ON
- APU Bleed Switch: AUTO
- FWD, AFT Outflow Valve Switch: AUTO

- Landing Altitude Selector: IN
- Right Wiper Selector: OFF
- Observer Audio ENT selector: AS DESIRED
- Map Light: AS DESIRED

- EFIS Control Panel: SET
- F/D Switches: BOTH OFF, THEN ON
- A/T Switches: OFF
- IAS/MACH Selector: SET
- A/P Disengage Bar: UP
- Bank Limit Selector: AUTO
- HDG/TRK Selector: SET
- Vertical Speed Selector: V/S
- Altitude Increment Selector: AS DESIRED
- Altitude Selector: SET
- LWR CTR (Display Select Panel): PUSH
- CANC/RCL Switch: PUSH

- Window 2 Left: CHECK
- Oxygen Mask/Regulator and Microphone: TEST/SET
- Shoulder Heater Control and Foot Heater Selector: AS DESIRED
- FWD Panel Light and Display Brihtness Control: ADJUST

- NAV Source Switch: OFF
- DSPL CTRL Source SwitchL OFF
- Air Data/ATT Source Switch: OFF
- Clock: CHEC/SET
- PFD: CHECK
- ND: CHECK
- Brake Source: CHECK
- Brake ACCUM Gauge: CHECK
- Inboard DSPL Selector: NAV/MFD
- Heading Reference Switch: NORMAL

- Standby Attitude Indicator: CHECK
- Standby Airspeed Indicator: CHECK
- Standby Altimeter: SET

- GND PROX G/S Light: OFF
- GND PROX Flap OVRD Switch: OFF
- GND PROX Gear OVRD Switch: OFF

- Landing Gear Lever: DOWN
- Altenate Gear Switch: NORMAL
- Autobrake Selector: RTO
- FMC Selector: AUTO
- Center Panel DSPL CTRL Switch: OFF
- CTR PNL Brightness Knobs: AS DESIRED
- Parking Brake: SET

- ALTN Pitch Trim Levers: NEUTRAL
- Speed Brake Lever: DOWN
- Throttles: CLOSED
- Reverse Thrust Levers: DOWN
- Flap Lever: CHECK
- ALTN Flaps Arm Switch: OFF
- ALTN Flaps Selector: OFF

- Fuel Control Switches: CUTOFF
- Stab Switches: NORMAL
- ENG Bottle 1,2 Disch Lights: OFF
- Engine Fire Switches: IN

- Left Radio Tuning Panel: VHF L or HF L
- Captain's Audio Control Panel: SET
- Weather Radar: TEST
- Center Radio Tuning Panel: VHF C
- Observer Audio Control Panel: SET AS DESIRED
- Flight Deck Door Switch: AS DESIRED
- OBS Audio Selector: NORMAL
- Interphone Handset: CHECK
- Flight Deck Printer: CHECK

- Rudder Trim: ZERO
- Aileron Trim: ZERO
- Center CDU: CABIN DIRECTORY
- Transponder Panel: SET

- Evacuation Signal Switch: OFF
- Floor Lights Switch: AS DESIRED
- Aisle Stand Light Control: AS DESIRED

- Seat: ADJUST 
- Rudder Pedals: ADJUST 
- Seat Belt/Shoulder Harness: ADJUST

- Cockpit Preparation - CAPTAIN: COMPLETED

____________________________________
Exterior Inspection

(During walk around, check the following for abnormal conditions:)

1. Left Mid Fuselage:
- Pack Inlet and Exhaust
- Negative Pressure Relief Vents
- Wing Illumination Light
- Static Ports
- Positive Pressure Relief Valves
- Forward Outflow Valve
- Crew Oxygen Thermal Discharge Disc

2. Left Forward Nose:
- L Pitot Probe
- L Ice Detector Probe
- TAT Probe
- L AOA Probe

3. Nose Section/Gear Area:
- Windshield Wipers
- Randome and Latches
- Forward Access Door
- Nose Gear Strut Extension
- Nose Down Lock Pin
- Nose Wheel Tires
- Steering Cables
- Main E & E Access Door
- APU Control Panel
- Steering Safety Pin

4. Right Forward Nose:
- Center Pitot Probe
- Right Ice Detector
- Right Pitot Probe
- Right AOA Probe
- External Power Door

5. Right Mid Fuselage:
- Forward Cargo Door
- Static Ports
- Pack Air Inlets and Outlets
- Wing Illumination Light

6. Right Wing Area and Engine:
- Landing Light
- Taxi and Turnoff Light
- Engine Strut
- Thrust Reverser and Sleeve
- EEC Static Ports
- Cowling and Fasteners
- Fan Blades
- PT2 Probe
- Reverser Blocker Doors
- AFT Fan Blades
- Wing Under Surface Area
- Leading Edge Slats and Flaps
- Fueling Adapter Panel
- Fuel Vent Scoop
- Navigation Lights
- Strobe Lights
- Static Discharge Wicks
- Aileron and Flaperon
- Fuel Jettison Nozzle
- Inboard and Outboard Flaps and Flap Drives

7. Right Main Gear: 
- Wheels and Tires
- Landing Gear Strut Extension
- Down Lock Braces
- Down Lock Safety Pin
- Gear Doors- CLOSED
- Gear Uplatch
- Hydraulic Leaks

8. Right AFT Fuselage:
- RAT Door
- Drain Mast for APU Fuel Line Shroud and Center Wing Dry Bay
- AFT Cargo Door
- Bulk Cago Door
- Static Ports

9. Tail Area:
- Lower Fuselage Structure and Tail Strike Sensor
- Static Ports
- APU inlet Door
- APU Oil/Fuel Drain
- APU Access Door
- Vertical/Horizontal Surfaces
- Static Discharge Wicks
- Top Surface of Both Wing and Tail
- APU Exhaust
- Strobe Light

10. Left AFT Fuselage:
- AFT Outflow Valve
- Water Drains, Service Doors, Waste Vents
- Air Demand Pump Exhausts (2)

11. Left Wing Area and Engine:
- Inboard and Outboard Flaps and Flap Drives
- Fuel Jettison Nozzle
- Aileron and Flaperon
- Static Discharge Wicks
- Strobe Light
- Navigation Lights
- Fuel Vent Scoop
- Fueling Adapter/Control Panel
- Leading Edge Slats and Flaps
- Wing Under Surface Area
- AFT Fan Blades
- Reverser Blocker Doors
- PT 2 Probe
- Fan Blades
- Cowling and Fasteners
- EEC Static Ports
- Thrust Reverser and Sleeve
- Engine Strut
- Taxi and Turnoff Light
- Landing Light

- Exterior Inspection: COMPLETE

____________________________________
Cockpit Preparation - First Officer

- Cockpit Voice Recorder: TEST
- Second Observer Audio Control Panel: CHECK
- Exterior Lights: AS REQUIRED
- Map Light: AS DESIRED

- EFIS Panel: SET
- Window 2 Right: CHECK
- Oxygen Mask/Regulator and Microphone: TEST/SET
- Shoulder Heater Control and Foot Heater Selector: AS DESIRED
- FWD Panel Brightness Controls: ADJUST

- NAV Source Switch: OFF
- DSPL CTRL Source Switch: OFF
- Air Data/ATT Source Switch: OFF
- Clock: CHECK/SET
- PFD: CHECK
- ND: CHECK
- Inboard DSPL Selector: NAV/MFD

- Radio Tuning Panel: VHF R or HF R
- Audio Control Panel: SET
- Left and Right HF Radios: CHECK
- ATIS: OBTAIN

- Seat: ADJUST
- Rudder Pedals: ADJUST
- Seat Belt and Shoulder Harness: ADJUST

- Cockpit Preparation - First Officer: COMPLETED

____________________________________
Company COMM and FMC Initialization - First Officer

- MFD, CO COMM (ACARS): ACCOMPLISH 
- CDU FMC Initialization: VERIFY
- CDU, PERF Init Page: SELECT, VERIFY, ENTER 
- CDU, Thrust Limit Page: SELECT, VERIFY, ENTER
- CDU, Takeoff REF Page: SELECT, VERIFY, ENTER 
- CDU, NAV RAD Page: SELECT
- CDU, NAV Data Page: SELECT
- CDU, VNAV Climb Page: SELECT, VERIFY, ENTER

- Company COMM and FMC Initialization - First Officer: COMPLETED

____________________________________
FMC Navigation Verification

- Present Position: VERIFY
- Route Entries: VERIFY
- (C, F/O) Class II NAV Procedures: ACCOMPLISH
- PERF, Thrust, Takeoff Entries: VERIFY
- (C) Verifcation Process: CONFIRM COMPLETE

- FMC Navigation Verification: COMPLETED
____________________________________
Final Cockpit Preparation

- (F/O) Fuel Sheet, Fuel Quantity: VERIFY/OBTAIN
- (F/O) ATC Clearance: OBTAIN
- (C, F/O) PERF, Thrust, Takeoff Data: REVIEW/SET
- (C, F/O) CDU NAV RAD: TUNE AS REQUIRED
- (C) IAS/MACH Selector: SET
- (C) Heading Selector: SET
- (C) Altitude Selector: SET
- (C, F/O) Departure Briefing: ACCOMPLISH
- (C) Seat Belts Switch: ON

To avoid unwanted fluid transfer, turn on hydraulic pumps in the following sequence: 
- (C) Right Electrical Demand Pump: VERIFY AUTO
- (C) C2 and C1 Primary Pump Switches: ON
- (C) Left Electrical, C1 and C2 Air Demand Pump Selectors: AUTO
- (C) Left and Right Fuel Pump Switches: ON

If center tank contains fuel:
- (C) Center Fuel Pump Switches: ON

- (C, F/O) Left, Right Inboard DSPL Selectors: SET
- (C) Stabilizer Trim: SET
- (C) Cockpit Door: LOCK
- (F/O) CANC/RCL Switch: PUSH

- (C, F/O) Final Cockpit Preparation: COMPLETED

____________________________________


____________________________________
	NORMAL PROCEDURES
____________________________________
Before Pushback Checklist

- (C) Doors: CLOSED
- (C) Cabin Preparation: VERIFY CABIN READY
- (F/O) Beacon Switch: ON
- (F/O) Pushback Clearance: OBTAIN

- (C, F/O) Before Pushback Checklist: COMPLETED

____________________________________
Preparation for Engine Start Checklist

- (F/O) Beacon Switch: CONFIRM ON
- (F/O) CANC/RCL Switch: PUSH

- (F/O) Preparation for Engine Start Checklist: COMPLETED

____________________________________
Engine Start Checklist

After clearance to start engines is received:
- (C) Engine Start: COMMAND
- (F/O) Secondary Engine Indications: DISPLAY
- (F/O) Start/Ignition Selector(s): START
- (F/O) Fuel Control Switch(es): RUN

- (C, F/O) Engine Indications: MONITOR
- (C, F/O) Engine Start Checklist: COMPLETED

____________________________________
After Start Checklist

- (C, F/O) Engine Indications/EICAS: MONITOR
- (C) Electrical Transfer: VERIFY
- (C) External Power: DISCONNECTED
- (C) APU Selector: OFF
- (C) Engine Anti-Ice Switches: AUTO/ON
- (F/O) CANC/RCL Switch: PUSH

After acknowedging the salute, but before taxi:
- (C, F/O) Audio Panels: SET
- (F/O) Taxi Clearance: OBTAIN

- (C, F/O) After Start Checklist: COMPLETED

____________________________________
Taxi Out Checklist

- (F/O) Flaps: SET
- (C, F/O) Flight Controls: CHECK
- (F/O) MFD CO COMM (ACARS): CHECK
- (PF) Inboard Display Selector: NAV
- (C) LNAV (as required): ARM
- (C) VNAV (as required): ARM

- (C, F/O) Taxi Out Checklist: COMPLETED

____________________________________
Before Takeoff Checklist

- (F/O) Route Changes (if appropriate): ENTER
- (F/O) Final Weights: ENTER
- (F/O) Takeoff Performance: CONFIRM
- (F/O) Stabilizer Trim (if appropriate): SET
- (C, F/O) Before Takeoff Checklist: COMPLETE EXEPT FINAL ITEMS

When cleared onto active runway (final items):
- (F/O) Transponder: TA or TA/RA
- (C) A/T Switches: ARM
- (F/O) CANC/RCL Switch: PUSH

(C, F/O) Before Takeoff Checklist: COMPLETED

____________________________________
Takeoff Checklist

When plane is in the active runway environment (crosses the "hold" line):
- (F/O) Wing Lights: ON
- (F/O) Strobe Lights: ON

When takeoff clearance is received:
- (C) Landing Lights: ON
- (PF, PNF) Parking Brake: RELEASE
- (PF) Takeoff Thrust: SET
- (PNF) TP/GA Switch(es): PUSH
- (PNF) Engine indications: MONITOR
- (PNF) Airspeeds: CALL OUT
- (PF) Initial Climb: ESTABLISH
- (PF, PNF) Positive Climb: ANNOUNCE
- (PNF) Landing Gear Lever (on order): UP

- (PNF) Takeoff Checklist: COMPLETED

____________________________________
After Takeoff Checklist

- (PNF) Heading (in order) AS REQUIRED
- (PF, PNF) Appropriate Noise Abatement Profile: ACCOMPLISH
- (PNF) A/P Engage Switch (on order): PUSH
- (PNF) Flaps (on order): RETRACT
- (PNF) Thrust: MONITOR
- (PNF) Engine Anti-Ice: AUTO

- (PNF) After Takeoff Checklist: COMPLETED

____________________________________
Climb Checklist

- (PNF) Cleared Altitude: SET
- (PF) Cleared Altitude: VERIFY
- (C) No Smoking Selector: AUTO/ON
- (C) Seat Belts Selector: AUTO/ON
- (PNF) VNAV (if not previously selected): ENGAGE
- (PNF) LNAV (if not previously selected): ENGAGE
- (PF) ECON Climb (at 10,000ft): VERIFY ACTIVE
- (C, F/O) Altimeters: SET AND ANNOUNCE QNE
- (C) Landing Lights (18,000ft): OFF
- (F/O) Wing Lights: (18,000ft): OFF
- (PF) Top of Climb (TOC): VERIFY DISPLAYED

- (PNF) Climb Checklist: COMPLETED

____________________________________
Cruise Checklist

- (PF, PNF) Level Off: VERIFY
- (PF, PNF) Cruise Thrust: MONITOR
- (PF, PNF) Flight Progress: MONITOR
- (PF, PNF) Fuel Management: MONITOR
- (PNF) Date Of Last Autopilot Approach and Autoland: CHECK
- (PNF) CO COMM (ACARS): ACCOMPLISH
- (PNF) Cleared Altitude: SET
- (PF) Cleared Altitude: VERIFY

- (PNF) Cruise Checklist: COMPLETED

____________________________________
Approach Descent Checklist

- (PNF) ATIS: OBTAIN
- (PF, PNF) Arrival Entries: SELECT, ENTER, VERIFY
- (PNF) DEP/ARR Page: COMPLETE
- (PNF) Legs Page: CHECK/COMPLETE
- (PNF) NAV RAD Page: ENTRY/VERIFY
- (PNF) Approach REF Page: COMPLETE
- (C, F/O) Approach/Landing Briefing: ACCOMPLISH
- (C) Seat Belt Selector: ON
- (PNF) CANC/RCL Switch: PUSH
- (C) Autobrake Selector: AS REQUIRED
- (C) Landing Lights (18,000ft): ON
- (F/O) Wing Lights: (18,000ft): ON
- (PNF) Approach Descent Checklist: COMPLET to TRANSITION LEVEL

When crossing Transition Level:
- (C, F/O) Altimeters: SET/ANNOUNCE QNH
- (PNF) Cabin Notification: ACCOMPLISH
- (C) No Smoking Selector: ON

- (PNF) Approach Descent Checklist: COMPLETED

____________________________________
Final Descent Checklist

- (PF, PNF) Flight/NAV Instruments: CHECK
- (PF, PNF) Autoflight Systems: AS REQUIRED
- (PNF) Flaps (on order): EXTEND
- (PNF) Landing Gear Lever (on order): DOWN
- (C) Speed Brake Lever: ARMED

- (PNF) Final Descent Checklist: COMPLETED

____________________________________
Landing Roll Checklist

- (PF, PNF) Touchdown/Rollout: MONITOR
- (PNF) Speed Brake Lever: MONITOR
- (PF) Reverse Thrust: AS REQUIRED
- (PNF) Engine Indications: MONITOR
- (PNF) Airspeed: MONITOR
- (PF) Reverse Lever: FORWARD IDLE
- (PF) Brakes: AS REQUIRED

- Landing Roll Checklist: COMPLETED

____________________________________
Taxi In Chcklist

When airplane is clear of active runway environment (crosses the "hold" line): 
- (C) Landing Light Switches: OFF
- (C) Runway Turnoff/Taxi Light Switches: AS REQUIRED
- (C) A/T Arm Switches: OFF
- (C) Left F/D Switch: OFF
- (C) Speed Brake Lever: DOWN
- (F/O) APU (on order): START
- (F/O) Engine Anti-Ice Selectors: AS REQUIRED
- (F/O) Wing Lights Switch: AS REQUIRED
- (F/O) Strobe Lights Switch: OFF
- (F/O) Right F/D Switch: OFF
- (F/O) WXR Radar Switches: OFF
- (F/O) Autobrakes Selector: OFF
- (F/O) Flaps: RETRACT
- (F/O) Stabilizer Trim: 7 UNITS
- (F/O) Transponder: STANDBY

- (F/O) Taxi In Checklist

____________________________________
Parking Checklist

- (C) Parking Brake: SET
- (C) Seat Belts Selector: OFF
- (C) Electrical Power: ESTABLISH
- (F/O) Fuel Control Switches (on order): CUTOFF
- (F/O) Beacon Light Switch: OFF
- (C) Anti-Ice: VERIFY OFF
- (C) Fuel Pump Switches: OFF
- (C) All Hydraulic Pumps (exept L, R, ENG): OFF
- (C) Window Heat: OFF
- (C) Emergency Lights Switch: OFF
- (C) Left Audio Selector Panel: SET
- (F/O) Exterior Lights: OFF
- (F/O) CDU NAV RAD Page: SELECT
- (F/O) CDU NAV DATA Page: SELECT
- (F/O) ADIRU Logbook Data: RECORD
- (C, F/O) Microphone Selector: FLIGHT
- (F/O) MFD Company COMM (ACARS) Accomplish
- (C, F/O) Indicator, Display and Instrument Lights: DIM

- (C, F/O) Parking Checklist: COMPLETED

____________________________________
Secure Checklist

- (C) ADIRU Switch: OFF
- (C) Pack Selectors: OFF
- (C) RECIRC Fans: OFF 
- (C) APU/EXT PWR Switches: OFF 
- (C) APU Selector: OFF 

2 minutes after moving APU selector to OFF:

- (C) Battery Switch: OFF

____________________________________


____________________________________
	IMPORTANT NOTES
____________________________________
* The Pilot Series Boeing 777-200 Checklist Full Version for FS2000. 

* Checklist for Boeing 777-200 made by Chris van Bijlert.
  Can also be used on all Boeing 777-100s and 777-300s.
  Derived from "meriweather.com's Flight Deck Simulations and Home Away from Home Web Site"
  Webmaster: Jerome Meriweather. http://www.meriweather.com
  Visit The Official Pilot Series Checklist Website: 
  http://fly.to/pilotserieschecklist
  Email me: chrisvanb@geocities.com

* Feel free to upload this checklist along your own
  freeware aircraft, as long as you limited it to one single 
  aircraft at a time. If you want to use this checklist on
  more than one aircraft at a time please contact me. 
  But do always keep this piece of text on it 
  and credit the designer (me!).
  When downloading and using this checklist you automaticly 
  agree with the Copyright & Use Notice as stated in the 
  documentation and on the website.

* Copyright (C.) Chris van Bijlert and Jerome Meriweather.