*******************************Piaggio P180 AVANTI************************

                         PILOT OPERATING HANDBOOK ADDENDUM

GENERAL WARNINGS
---------------------

To obtain correct perfomances under all flight phases, pilots must operate the acft as follow

- DO NOT EXCEED RED LINE ON ITT INSTRUMENT

- NEVER EXCEED 95% TORQUE FOR NORMAL OPERATIONS (two engines operating). 
For emergencies, or in case of ONE ENGINE OUT, MAX 103% CAN BE ACHIEVED ( MAX 3 MIN )

- USE 2000 RPM FOR TAKE OFF, CLIMB AND MAX. CRUISE SPEED. MAX SPEED IS OBTAINED 
APPLYNG FULL THROTTE @ 28,000 - 29,000 FT.
ABOVE THIS ALTITUDE FULL THROTTLE IS PROHIBITED BECAUSE  MAX PROPELLER RPM CAN
BE EXCEEDED AND PROPELLER PITCH IS NO MORE ADJUSTABLE. USE BOTH PITCH AND THROTTLE
TO STAY WITHIN OPERATING LIMITS.

- MAX OPERATING SPEED IS 260 KIAS / 0.68 Vne  0.70 M

