* TNC Init file for Kantronics
!Kantronics TNC File
int terminal

B E 0
DIGI on
EXP on
FLow off
FUll off
HEA off
LFadd off
LFSup ON
AUTOLF off
MCOM off
MON ON
MResp OFF
MRPt on
MSTamp off
MXMit off
NEWmode off
PACLen 128
PID off
SCR 0
* B E 0 MUST BE SET to 0 or both APRS and your TNC will send BCNS
* Which will alternate in EVEYONES L and A lists, and FILL UP THEIR LOGS
* Do NOT set B E to anything other than 0! (while APRS is running!)
*
* APRS internally sets the following commands:  UNPROTO, MYCALL, MYA RELAY
* IF HF then APRS will set:  MAX 1,  AX25lvl2 off,  MYAlias ECHO

