#######################################################################
#	IF THIS FILE LOOKS MESSED UP, YOU MAY NEED TO ADD LINE FEEDS
#
#	You may edit this file, however WinAPRS wont recongize the file
#	until the next time you restart
#	Obviously, lines starting with '#' are comments
#	Fields must be seperated by TAB
#
#	NOTE: the default port for TELNET is 23, most APRS servers do NOT
#	use 23, the port MUST be specificed for all of the entries, even
#	if they are port #23
#
#	If your environemnet uses a PROXIE server, uncomment the "PROXIE"
#	line and enter your information. The proxie statement can be anywhere
#	and applies for ALL of the entries.
#
#	NOTE ! ! ! ! !!
#	The PROXIE code has NOT been thoroughly tested, please let me know if it
#	doesnt work.  It will ONLY work IF your proxie simply is looking for
#	"www.aprs.net 10151<CR>", if it needs passwords or anything else, the
#	proxie mode will NOT work
#
#######################################################################
#PROXIE	kb2ear.aprs.net	5071
www.aprs.net	10151	Southern Florida, USA Composite
www.aprs.net	14579	(Southeast FL) APRServe/Macintosh
www.wa4dsy.radio.org	14579	Atlanta GA,
kb2ear.aprs.net	14579	Central NJ, 145.790 MHz only 
kb2ear.aprs.net	6261	Central NJ,HF only
kb2ear.aprs.net	14580	Central NJ,145.79 + HF
#www.ne1h.radio.org	14579	Atlanta, GA aprsmon/Linux
#nt4l.aprs.net	14579	middle TN APRServe/Macintosh
#sboyle.slip.netcom.com	14579	San Francisco, CA	
