* These cmds will be executed each time you start APRS or hit alt-SETUP-TNC
* The first group are unique to the AEA TNC's.  The second are standard
* Some EARLY PK-12's must have BBSMSGS ON, but OFF is preferred if it works

EXP on
ALFP off
ACRD 0
ALFD off
BBSMSGS off
MON 2
MXmit off
Mto ALL
MDIGI on
DFrom all

MCOM off
Echo off
FLow off
FULL off
PACLen 128
MSTamp off
NEWmode off
MRPT ON
HEA off
DIGi on
B E 0
* If you do not set B E 0 then both APRS and your TNC will both send BCNS
* Which will alternate in EVEYONES L and A lists, and FILL UP THEIR LOGS
* DIrectory.  Do NOT set B E to anything other than 0!

